Steps to replace tube in the BE FM TX’s

**1.    Shut off all AC power to the transmitter.**

**2.    Open front panel door to get access to the tube.**

**3.    Unhook the banana plug (High Voltage plug) from the chimney.**

**4.    Loosen the hose clamp on the bottom of the chimney.**

**5.    Pull the chimney up through the plexiglass shelf and then turn it so the stubs can rest on the shelf.**

**6.    Reach in and carefully put the tube straight and remove it from the socket.**

**7.    Inspect the finger stock in the socket to make sure they are ok and not all broke off.**

**8.    Install the new tube and gently push down to make sure it is seated good.**

**9.    Set the chimney back in place over the tube.**

**10.  Tighten down the hose clamp.**

**11.  Plug the banana plug back into the chimney.**

**12.  Close the front panel doors and secure the screws.**

**13.  Apply AC power to the transmitter and you will be ready to go.**

**If you need any help or have questions give us a call at 217-224-9600.**